****

Product Specifications

**Light Weight Pipe Anchor.**

1. General
   1. Provide Light Weight Anchor Clamps pipe guides as indicated on project plans or as required.
   2. Light Weight Anchor Clamps are designed for use with low load expansion joints such as the Metraloop.
2. Products
   1. Light Weight Anchor Clamps shall be **PA Anchor** as manufactured by The Metraflex Company®, Chicago, IL.
   2. PA Anchor clamp shall be fabricated from ASTM A-36 carbon steel.
   3. All surfaces of anchor shall have Alkyd corrosion resistant paint.
   4. PA Anchor shall feature two pipe clamps.
   5. PA Anchor shall be rated for the following loads.

Size Load Rating

2” 80 lbs.

2.5” 85 lbs.

3” 95 lbs.

4” 125 lbs.

6” 210 lbs.

8” 265 lbs.

10” 290 lbs.

12” 395 lbs.

1. Execution
   1. Installation shall be in accordance with manufacturer’s printed instructions.
   2. PA Anchors are not intended for use with bellows or rigid pipe expansion assemblies.