**Note to users: items shown in red indicated edits / selections that need to be made to tailor the specification for the application.**

**Threaded Bronze Center Guided Silent Check Valve.**

1. **General:**
   1. Threaded bronze center guided check valves shall be installed where shown on plans or required by equipment manufacturers.
2. **Product:**
   1. Threaded Bronze Center Guided Silent Check Valve shall be model **“BSN"** as manufactured by The Metraflex Company®, Chicago, IL.
   2. Materials:
      1. Check valve body shall be bronze conforming to ASTM B584 Alloy C30300.
      2. Check valve trim.
         1. Check valve disk shall be PTFE.
         2. Check valve spring shall be Type 316 Stainless steel.
3. **Execution:**
   1. Bronze check valves shall be installed in accordance with manufacturer’s recommendations and contact requirements.



Product Specifications