 **Riser Guide, Silent Style.**

Product Specifications

1. General
   1. Provide Silent Style Riser Pipe Guides as indicated on project plans or in accordance with engineering calculations.
   2. EJMA standards may not be applicable to risers.
2. Products
   1. Pipe guides shall be style “**PGQ Riser Guide**” as manufactured by The Metraflex Company®, Chicago, IL.
   2. Guide shall be made up of a housing with base plate, T slide and urethane load bearing isolator.
   3. Guide shall be manufactured from ASTM A-134 carbon steel.
   4. Piping shall be connected to slide assembly with clamps. Copper pipe shall utilize dielectric inserts.
3. Execution
   1. Install and guide per manufacturer’s installation instructions and Mechanical Contractors Association of America “Guidelines for Quality Piping Installations”.