**Split Disk Wafer Style Check Valve.**

1. **General:**
	1. Split disk style check valves shall be installed where shown on plans or required by equipment manufacturers.
	2. Check valve shall be certified to be in conformance with NSF 372.
2. **Product:**
	1. Wafer Style Center Guided Silent Check Valve shall be model **“CVXXK"** as manufactured by The Metraflex Company®, Chicago, IL.
	2. Materials:
		1. Check valve body shall be ASTM A126 B Cast Iron with fusion bonded epoxy coating.
		2. Check valve disk shall be CF8 stainless steel.
		3. Check valve spring shall be Type 304 Stainless steel.

.

1. **Execution:**
	1. Split disk wafer style check valves shall be installed in accordance with manufacturer’s recommendations and contact requirements.
	2. Check valve shall be installed between ASME B16.1 flanges.
	3. Installer shall insure there is no interference between check valve and adjacent equipment.



Product Specifications